## QMedia v1.5 | ## Introducing QuickTime

Home | Time management | Tracks | QTVR movies | Standard properties | Controller Properties | VR properties | Track properties | Editing

## VR Movie Properties

Default view | The view that is displayed when a QTVR movie is initially opened.
Current node | The ID of the current VR node.
Pan angle | The pan angle, expressed in degrees.
Pan angle range | The minimum and maximum values for pan angle (set by the author).
Tilt angle | The tilt angle, expressed in degrees.
Tilt angle range | The minimum and maximum values for tilt angle (set by the author).
Field of view | The viewing angle, expressed in degrees.
Field of view range | The minimum and maximum values for field of view (set by the author).
View center | The coordinates of the object's center in an object node. This property does not exist in panoramic views.
View center range | The minimum and maximum values for view center (set by the author).

### Node Properties

Type | A 4-character code identifying the type of the node. Currently, QTVR supports two types of nodes: panoramas ("pano") objects ("obje")
ID | A unique number that identifies the node within the VR movie. Node IDs are assigned by the authoring software.
Name | The name of the node. Set by the movie's author.
Comment | The node's comment. Set by the movie's author.

### Hot Spot Properties

Type | A four-character code identifying the type of the hot spot. Currently, QTVR supports the following types of nodes: link hot spots ("link") URL hot spots ("url ") undefined hot spots ("undf") An application can define and use its own hot spot types.
ID | A unique number that identifies the hot spot within the node. Hot spot IDs are assigned by the authoring software.
Name | The name of the hot spot.
Link destination | The link destination of the hot spot. This can be a node ID or a URL.