## QMedia v1.5 | ## Using QMedia

Home | Playback | Internet delivery | Grabbing

Requirements | How grabbing works | Grabber setup

## Sequence Grabbing Requirements

| MacOS X | Windows
Machine | Intel-based Mac recommended. | Intel Core Duo or better.
Video input | PCI video capture board or USB camera or FireWire camera with appropriate driver (VDIG) | PCI video capture board or USB camera or FireWire camera with appropriate WDM driver supported by WinVDIG (see below).
Audio input | Built-in or external audio input. | DirectSound compatible sound card (natively supported by QuickTime for Windows).
System software | MacOS 10.4.10 or later QuickTime 6 or later | Windows XP/Vista QuickTime 6 or later

Windows drivers

WinVDIG http://www.vdig.com/WinVDIG/

WinVDIG is a video digitizer that bridges the gap between QuickTime and Windows capture drivers. WinVDIG creates virtual VDIGs for installed WDM (Windows Driver Model) and VfW (Video for Windows) capture drivers, allowing QuickTime-based applications to capture video using hardware that lacks QuickTime support (a VDIG).

MacOS X drivers

IOExperts http://www.ioxperts.com/

IOXperts provide MacOSX native drivers for a large range of USB and FireWire cameras.

Macam http://webcam-osx.sourceforge.net/

Macam by Matthias Krauss is an open-source video digitizer for USB-based cameras on MacOSX. The project initially supported a few Philips models, but it has evolved to cover a range of models from other manufacturers as well.